## Pre-Flight Checklist

|  |
| --- |
| RPIC:  |
| Visual Observer(s): | UAS Model: DJI Mavic 2 |
| Location: |
| Check | Item | Notes |
|  | Clear Area |  |
|  | Check Weather Conditions |  |
|  | Check Area for Obstructions |  |
|  | Setup Launch Location |  |
|  | Place Aircraft into Position |  |
|  | Remove Gimbal Cover |  |
|  | Power on Transmitter |  |
|  | Transmitter Battery Level > 20% |  |
|  | Rotate Transmitter Antennas |  |
|  | Start DJI Go4 |  |
|  | Power on Aircraft  |  |
|  | Aircraft Battery Level > 90% |  |
|  | No warnings on screen |  |
|  | Aircraft Memory Card installed |  |
|  | Memory Card has sufficient space |  |
|  | Check Mode set to ‘P’ |  |
|  | Announce ‘Aircraft Ready’ |  |
|  | Instruct VO to position |  |
|  | Check for Air Traffic |  |
|  | Announce ‘Ready to Launch’ |  |
|  | Wait for Crew Confirmation |  |
|  | Announce ‘Launching’ |  |
|  | Initiate Launch |  |
|  | Hover in place for a few seconds |  |
|  | Start Flight Routine |  |